





That is a theoretical maximum number computed by multiplying the memory bus width by the max clock rate:  
  
2505MHz \* 2 (DDR) \* 384 bits / 8bits per byte = 240GB/s.